http://zd1211.ath.cx/

Loading Driver
--------------

# modprobe -v zd1211
# lsmod - you should see zd1211 loaded (see dmesg otherwise)
# ifconfig wlan0 up (iwconfig will not work otherwise)
# iwconfig wlan0 essid youressid
# dhclient wlan0 (or ifconfig.../route... for static IP) - use dhcpd or pump if your distribution does not feature dhclient

Configuration
-------------

AP Master mode

* /etc/network/interfaces

auto wlan0
iface wlan0 inet static
        address 192.168.1.1
        netmask 255.255.255.0
        network 192.168.1.0
        broadcast 192.168.1.255
        wireless_essid myessid
        wireless_channel 7
        wireless_mode master
        wireless_rts 512
        wireless_frag 512
        wireless_key secretkey
        pre-up /etc/init.d/dhcp3-server stop
        post-up iwpriv wlan0 set_mac_mode 1
        post-up /etc/init.d/dhcp3-server start


